PAVING CATEGORY:
Pavement Resurface (Overlay) Service
Proposed Area:  This proposal is based on approximately {area_of_paving} {unit}.
Contouring:  In order to maintain a flush transition and uniform thickness from the new pavement to the match points, we will mill and profile the existing asphalt pavement where it meets utility lids, concrete aprons, dumpster pads, etc. to prepare for the proposed asphalt pavement surface.
Sweeping:  We will sweep all surfaces to be paved clear of loose materials.
Tack Coat:  We will apply a tack coat adhesive at 0.05 gallons/square yard.
Leveling Course:  We will manufacture, furnish and machine pave hot-mix asphalt to wedge and fill low and depressed areas.  
Paving:  We will manufacture, furnish and pave {depth_of_paving} inches of average compacted thickness hot-mix asphalt pavement consisting of {asphalt surface} surface course material.
Car Stops:  This proposal includes setting aside {number_of_parking_blocks} car stops and re-pinning upon the completion of paving.  We will do everything possible not to damage the existing car stops, however if they are currently damaged moving them could possibly cause future damage.
Pavement Markings:  This proposal includes painting the parking stalls and symbols per existing layout and color.
Please Note:  We are not responsible for reflective cracking that could occur due to the condition of the existing underlying pavement.   It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization per crew.  If work requires multiple mobilizations to be completed, not at the direction of us, additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date.
Remove and Replace Reconstruction Service
Proposed Area:  This proposal is based on approximately {measurememt_of_total_area} {unit_of_measurement}.
Removal/Dispose of Existing Material:  We will excavate and remove the existing asphalt pavement to expose and inspect the existing underlying aggregate base course. Excavated materials will be taken to recycling facility for processing.
Proof Roll: If needed a proof roll the existing underlying aggregate base course will be performed with the client to verify that a stable structural base is present.  If there are areas discovered that are failing it will be brought to the client’s attention and approval will be required at that time. 
Ready To Pave Conditions:  Proposed area will be properly fine graded by others to a ready to pave condition and to have passed an owner sanctioned proof roll.
Crushed Aggregate Base Course (CABC):  Upon the completion of a successful proof roll we will top-dress the existing underlying aggregate base course with CABC material to re-establish the existing drainage patterns.  (Proposal includes XXX Tons of CABC)
Fine Grading:  We will fine grade and compact the aggregate base course.
Paving:  We will manufacture, furnish and pave an average of  XX inches compacted thickness of  hot-mix asphalt pavement in two lifts consisting of  {asphalt_base inches} inches  {asphalt binder}, {oil type a} binder course material and{asphalt_surface_depth_in} inches of {asphalt surface}, {oil type b} surface course material. 
Unforeseen Conditions: In the event that the proof roll identifies "soft spots" we will charge $ XX.XX/Ton to stabilize the unsuitable base prior to the installation of the new base course and asphalt pavement.  Depth of additional excavation will be determined on-site, if needed, with company representative and client. 
Please Note:  The above will not be performed without Client's consent.


Pavement Markings:  This proposal includes painting the parking stalls and symbols per existing layout and color.
Please Note:  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization per crew.  If work requires multiple mobilizations to be completed, not at the direction of Wolf Paving, additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date.

Pulverize or Milling Pavement Reconstruction Service
Proposed Area:  This proposal is based on approximately {area_of_paving} {unit}.
Pulverizing:  This proposal includes Pulverizing the existing asphalt pavement and utilize as the proposed aggregate base course.  We will rough grade to maintain the existing drainage patterns and meet the abutting match points.
Sweeping:  We will sweep all surfaces to be paved clear of loose materials.
Tack Coat:  We will apply a tack coat adhesive at 0.05 gallons/square yard.
Proof Roll:  If needed a proof roll of the pulverized asphalt aggregate base course will be performed with client to verify that a stable structural base is present.  If there are areas discovered that are failing it will be brought to the client's attention and approval to move forward will be required at that time.   
Crushed Aggregate Base Course (CABC):  Upon the completion of a successful proof roll we will top-dress the existing underlying aggregate base course with CABC material to re-establish the existing drainage patterns.
Paving:  We will manufacture, furnish and pave an average of  XX inches compacted thickness of hot-mix asphalt pavement in two lifts consisting of {asphalt base binder} inches of asphalt binder , {base asphalt material}, {oi ltype a} binder course material and {depth_of_paving} inches, {surfaceasphaltmaterial}, {oiltypeb} surface course material.	
Pavement Markings:  This proposal includes painting of the parking stalls and symbols per existing layout and color.
Please Note:  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization per crew.  If work requires multiple mobilizations to be completed, not at the direction of us, additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date. 
Unforeseen Conditions:  In the event that the proof roll identifies "soft spots" in the base/subgrade; it will need to be stabilized.  We will charge $ XX.XX/Ton to stabilize the base prior to the installation of the new asphalt pavement.
Please Note:  The above will not be performed without Client's consent.











Full Depth Pavement Section Construction Service
Proposed Area:  This proposal is based on approximately {area_of_paving} {unit}.
Excavation:  We will excavate and remove the existing asphalt pavement and underlying aggregate base course to an average depth of (total_excavation_depth) inches below the finished elevation.  Excavated materials will be taken to recycling facility for processing. 
Proof Roll:  If needed a proof roll of the existing underlying subgrade will be performed with the client to verify that a stable structural base is present.  Areas discovered that are failing the proof roll shall be completely excavated, disposed off-site and backfilled with a new 3 inches crushed aggregate base course material.  
 Crushed Aggregate Base Course (CABC):  Upon the completion of a successful proof roll, furnish and place XX  inches of CABC material in the proposed asphalt pavement area. We will rough grade, compact with a vibratory roller and finish grade and compact the aggregate base course.
Paving:  We will manufacture, furnish and pave an average of  XX inches compacted thickness of hot-mix asphalt pavement in two lifts consisting   of {asphalt_base_inches}"  {asphalt binder}, {oil type a} binder course material and {asphalt_surface_depth_in}​" of {asphalt surface}, {oil type b} surface course material.
Pavement Markings/Handicap Signage Requirements:  This proposal includes painting the parking stalls and symbols per client's supplied pavement marking layout/diagram and color scheme.
Please Note:  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization per crew.  If work requires multiple mobilizations to be completed, not at the direction of us, additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2015 if this proposal is signed and returned within 30 days of the proposal date.
Unforeseen Conditions: In the event that the proof roll identifies "soft spots" we will charge $ XX.XX/Ton to stabilize the unsuitable base prior to the installation of the new base course and asphalt pavement.  Depth of additional excavation will be determined on-site, if needed, with a company representative and client. 
Please Note:  The above will not be performed without Client's consent.



Excavation Service 
Proposed Area:  This proposal is based on approximately {area_of_paving} {unit}.
Asphalt Pavement Excavation:  We will excavate and remove the existing asphalt pavement to expose and inspect the existing underlying aggregate base course.  Excavated materials will be taken to recycling facility for processing. 
Excavation Below Finished Elevation:  We will excavate and remove the existing asphalt pavement and underlying aggregate base course to an average depth of (total_excavation_depth) inches below the finished elevation.  
Please Note:  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization.  If work requires multiple mobilizations to be completed, not at the direction of us, additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date.





Aggregate Base Course Construction Service 
Proposed Area:  This proposal is based on approximately {area_of_paving} {unit}.
Crushed Aggregate Base Course (CABC):  We will furnish and place XX inches of 1-1/4" CABC material in the proposed asphalt pavement area.  We will water the CABC material to ensure maximum compaction.
Rough Grade and Compact:  We will rough grade and compact the crushed aggregate base course material to within 0.10' of the designed elevations.
This Proposal Includes:  The base course under the proposed concrete curb and gutter. 
This Proposal Excludes:  The base course under the proposed concrete flatwork.
Please Note:  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization.  If work requires multiple mobilizations to be completed, not at the direction of us, additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date.
Asphalt Pavement Construction Service 
Proposed Area:  This proposal is based on approximately {area_of_paving} {unit}.
Construction by Others:  If the pavement section aggregate base course is constructed by others, all base material will be on-site and graded to within 0.10' of the designed elevations and to have successfully passed a Client and Company sanctioned proof roll. If additional Crushed Aggregate is needed add $XX.XX/Ton to the project total for 1-1/4" crushed aggregate material to establish the proper elevations for the proposed asphalt pavement construction. 
Ready Pave Conditions:  Proposed area will be properly fine graded to a ready to pave condition and to have passed an owner sanctioned proof roll.
Fine Grading:  We will fine grade and compact the aggregate base course.
Paving:  We will manufacture, furnish and pave an average of XX inches compacted thickness of hot-mix asphalt pavement in two lifts consisting of {asphalt_base_inches} inches of {asphalt binder}, {oil type a} binder course material and {asphalt_surface_depth_in}​ inches of {asphalt surface}, {oil type b} surface course material.
Please Note:  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization.  If work requires multiple mobilizations to be completed, not at the direction of us, additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date.
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Milling and Pavement Reconstruction
Proposed Area:  This proposal is based on approximately {area_of_paving} {unit}.
Milling:  This proposal includes Milling to a depth of _XX__inches.
Sweeping:  We will sweep all surfaces to be paved clear of loose materials.
Tack Coat:  We will apply a tack coat adhesive at 0.05 gallons/square yard.
Proof Roll:  If needed a proof roll of the milled asphalt aggregate base course will be performed with the client to verify that a stable structural base is present.  If there are areas discovered that are failing it will be brought to the client's attention and approval to move forward will be required at that time.   
Crushed Aggregate Base Course (CABC):  Upon the completion of a successful proof roll we will top-dress the existing underlying aggregate base course with CABC material to re-establish the existing drainage patterns.
Paving:  We will manufacture, furnish and pave an average of  XX inches compacted thickness of hot-mix asphalt pavement in two lifts consisting of {asphalt base binder} inches of asphalt binder , {base asphalt material}, {oil type a} binder course material and {depth_of_paving} inches, {surface asphalt material}, {oil type b} surface course material.     
Pavement Markings:  This proposal includes painting of the parking stalls and symbols per existing layout and color.
 
Please Note:  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization per crew.  If work requires multiple mobilizations to be completed, not at the direction of us, additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date.
Unforeseen Conditions:  In the event that the proof roll identifies "soft spots" in the base/subgrade; it will need to be stabilized.  We will charge $ XX.XX/Ton to stabilize the base prior to the installation of the new asphalt pavement.
Please Note:  The above will not be performed without Owner's consent.









Fine Grading Option

Fine Grading Option:  We will fine grade and compact the CABC for the proposed pavement area which is approximately XXXXX Square Yards.

Construction by Others:  If the pavement section aggregate base course is constructed by others, all base material will be on-site and graded to within 0.10' of the designed elevations and to have successfully passed a Client and Company sanctioned proof roll. If additional Crushed Aggregate is needed add $XX.XX/Ton to the project total for 1-1/4" crushed aggregate material to establish the proper elevations for the proposed asphalt pavement construction. 

Please Note:  This proposal does not include staking and layout, subgrading (undercutting/filling) or base under any concrete structures.  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization.  If work requires multiple mobilizations to be completed, not at the direction of us, additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date.
ASPHALT REPAIR CATEGORY
Asphalt Excavation Repair
Proposed Area:  This proposal is based on {repair_locations} area(s), approximately {measurement} {area_unit} of deteriorated pavement.
Saw Cut and Excavate:  We will saw cut the perimeter of the repair area and excavate to a depth of {exc_depth} {exc_unit}.   Excavated materials will be taken to recycling facility for processing.
Proof Roll: If needed a proof roll the existing underlying aggregate base course will be performed with the client to verify that a stable structural base is present.  If there are areas discovered that are failing it will be brought to the owner’s attention and approval will be required at that time. 
Crushed Aggregate Base Course (CABC):  Upon the completion of a successful proof roll we will top-dress the existing underlying aggregate base course with CABC material to re-establish the existing drainage patterns.
Paving:  We will manufacture, furnish and pave an average of XX inches compacted thickness of hot-mix asphalt pavement in two lifts consisting of {asphalt_base_inches} inches  {asphalt binder} binder course material and{asphalt_surface_depth_in}​ inches of {asphalt surface} surface course material.
Please Note:  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization.  If work requires multiple mobilizations to be completed, not at the direction of us, additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date.
Unforeseen Conditions:  In the event that the proof roll identified "soft spots" are evident we will charge $ XX.XX/ton to stabilize the unsuitable base prior to the installation of the new asphalt pavement.
Please Note:  The above will not be performed without Owner's consent.






Asphalt Milling Repair
Proposed Area:  This proposal is based on approximately {measurement} {area_unit}.
Milling:  We will mill your pavement to the depth of {depth} {depth_unit}.  All millings and loose material will be removed from the site.
Paving:  We will manufacture, furnish and pave an average of XX inches compacted thickness of hot-mix asphalt pavement in two lifts consisting of of {asphalt_base_inches} inches  {asphalt binder} binder course material and{asphalt_surface_depth_in}​ inches of {asphalt surface} surface course material.
Please Note:  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization.  If work requires multiple mobilizations to be completed, not at the direction of us, additional mobilizations will be charged at:  $ XX 0/MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date.

Infrared Pavement Repair
Proposed Area:  This proposal is based on {repair_locations} area(s), approximately {measurement} {area_unit} of area requiring infrared pavement repair.
Infrared Process:  The infrared process consists of lowering the infrared heat chamber over the repair area for 15 to 20 minutes to heat the existing pavement without oxidation.  Once the repair area has been heated, scarifying with a rack to remove failed aggregate and an application of rejuvenator to replenish lost oils, due to oxidation, will take place.
Paving:  Additional hot-mix asphalt material will be applied to the area, while raking and grading it to the proper level and compacted.
Barricading:  Generally after a period of approx. 30 minutes the areas where infrared repair has taken place can be reopened to traffic.
Please Note:  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization.  If work requires multiple mobilizations to be completed, not at the direction of us, additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date.

Pot Hole Filling
Proposed Area:  We will remove loose material from the pot hole area and then install approximately {hot_mix_tons_to_install} tons of hot mix asphalt throughout the parking lot.
Paving:  We will level and fill pot holes throughout your parking area, shape and compact. 
Please Note:  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization.  If work requires multiple mobilizations to be completed, not at the direction of us, additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date.






Concrete Repair
Proposed Area:  This proposal for concrete repair is based on approximately {repair_in_sqft} sq. ft of deteriorated concrete.
Saw Cut and Excavate:  We will saw cut and excavate repair to a depth of {depth_of_repair} inches.
Concrete:  We will form, place and finish repair concrete to match existing surface texture and grid system and apply cure and seal.
Please Note:  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization.  If work requires multiple mobilizations to be completed, not at the direction of us, additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date.
SEALCOATING CATEGORY
Pavement Sealcoating
Proposed Area:  This proposal is based on approximately {area} {area_unit}.
Crackfilling Process:  We will clean out weeds as needed and apply vegetation killer to retard any weed growth in pavement.  Blow or sweep debris from the area to be sealed.  Clean out pavement cracks with compressed air to eliminate dust and debris that could inhibit bonding of sealant.  Dry cracks as needed to ensure 100% adhesion.  Seal cracks with federal specified ASTM-3405/ASTM-6690 Crafco Roadsaver 221 hot tar sealant.  Please Note:  This excludes heavily alligatored areas.  Crackfilling will not repair failed (spidered or alligatored) areas of existing pavement.
Sealing Process:  We will Spot-X any oil or chemical spillage as needed to aid in the adhesion of sealer to the pavement.  Using commercial grade asphalt emulsion sealcoat (1 to 2 lbs of silica sand/gallon and 2% latex additive), trim by hand all areas adjacent to garage doors, concrete, etc.  Apply on coat to entire area to fill pores and irregularities.  We will apply a second coat to entire area for maximum coverage.
Client's Responsibility:  It is the client’s responsibility to have all material, cars, equipment etc. removed from the area where the work will take place. Please review the attached Owner's Responsibility & Conditions page.
It is recommended that commercial grade pavement sealer be applied one year after initial pavement installation and then re-applied every 2 to 3 years (based on typical usage).  Sealer can help preserve and protect the asphalt from substances (gasoline, oil, hydraulic fluids, etc.) and oxidation that can breakdown the pavement stability as it loses its structural oils.
Please Note:  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization.  If work requires multiple mobilizations to be completed, not at the direction of us, additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date.










Crackfilling (Only)
Proposed Area: This proposal is based on approximately {measurement_} {area_unit}.
Crackfilling Process:  We will clean out weeds as needed and apply vegetation killer to retard any weed growth in pavement.  Blow or sweep debris from the area to be sealed.  Clean out pavement cracks with compressed air to eliminate dust and debris that could inhibit bonding of sealant.  Dry cracks as needed to ensure 100% adhesion.  Seal cracks with federal specified ASTM-3405/ASTM-6690 Crafco Roadsaver 221 hot tar sealant.  Please Note:  This excludes heavily alligatored areas.  Crackfilling will not repair failed (spidered or alligatored) areas of existing pavement.
Please Note:  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization.  If work requires multiple mobilizations to be completed, not at the direction of us, additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date.

Route the Cracks prior to Crackfilling

Crack routing creates a fresh clean side wall for better adhesion and creates a reservoir to maximize the amount of hot tar to be filled below the existing adjacent pavement surface.
Route the new cracks 1/4" and larger out to approximately 3/4" x 3/4" and dispose of the debris.
Please Note:  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization.  If work requires multiple mobilizations to be completed, not at the direction of us, additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date.

CONCRETE CATEGORY
Concrete Repair
Proposed Area:  This proposal for concrete repair have been identified throughout your area of approximately {_of_repair_areas} areas requiring concrete repair comprising {measurement_in_sqft} square feet.
Saw Cut, Excavate and Pour Concrete:  All areas will have the perimeter saw cut and excavated to a depth of {depth_of_repair} inches.  We will form, place and finish to match existing concrete.
Unforeseen Conditions:  When saw cutting concrete, there is a paste material that will form.  We have included the removal and cleanup of this by washing down existing storm drains.  In the event that this is not allowed, there may be additional costs.
Barricading/Caution Tape: All areas will be barricaded and/or taped before, during and after the project.  It is the owner’s responsibility to make sure all barricades remain effective after our crews leave the jobsite.
Please Note:  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization.  If work requires multiple mobilizations to be completed, not at the direction of us, additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date.




LINE STRIPING CATEGORY
PAVEMENT MARKINGS - NEW
Proposal Area:  This proposal includes painting the parking stalls and symbols per client's supplied pavement marking layout/diagram and color scheme.
Please Note:  All work will be performed so that there is minimal interruption to your facility.  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization.  If work requires multiple mobilizations to be completed, not at the direction of us additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date.

PAVEMENT MARKINGS – EXISTING
Proposed Area:  This proposal includes painting the parking stalls and symbols per existing pavement marking layout/diagram and color scheme.
Please Note:  All work will be performed so that there is minimal interruption to your facility.  It is the client’s responsibility to clear the proposed work area of any items that may prohibit crew efficiencies.  This proposal pricing is based on asphalt/grading to be completed in ONE mobilization.  If work requires multiple mobilizations to be completed, not at the direction of us additional mobilizations will be charged at:  $ XX /MOB for the grading crew and $ XX /MOB for the paving crew. The enclosed price is good for 2016 if this proposal is signed and returned within 30 days of the proposal date.

Pavement Markings- With Bollards
Proposal Area:  This proposal includes painting the parking stalls, symbols and bollards per client's supplied pavement marking layout/diagram and color scheme.
Please Note:  All work will be performed so that there is minimal interruption to your facility.
Below is previously used Text:
Proposed Area: This proposal is based on Parking Stalls {parking_stalls}  | Arrows {arrows} | Handicapped{handicapped} | Color Box Handicapped {handicapped_color_box} | Reserved {reserved_wording} | Fire Lane Wording {fire_lane_wording} | Lineal Feet Line other than striping {lineal_feet} | Curbing {curbing_lf} l.f | Exit/Enter{exitenter}.
Pavement Markings:  We will complete this project in {trips_to_complete} trips.  In the event that cars are not moved, sprinklers are left on or any other reason we are not able to complete the work on the scheduled day, there will be an addition trip charge of ${additional_trip_charge} per required trip.
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