Proposal to Include:

1. Disconnect and recover refrigerant from quantity (?) existing unit(s)
2. Remove unit and dispose of existing size ton per EPA regulations
3. Furnish and install quantity (1) size ton brand gas heating and electric cooling roof top unit(s)
a. Model number
b. Standard or high efficiency
c.  Economizer
d. Barmoetric relief or power exhaust
4. Furnish and install adaptor curb(s) if necessary
5. Crane and rigging
6. [bookmark: _GoBack]Gas piping reconnection using only black iron pipe
7. Line voltage wiring reconnection
8. Modify circuit breaker or fuse sizing if required
9. Furnish and install GFI within twenty feet of new unit if none existing
10. Reconnect control wiring
a. If currently controlled by a DDC control system:
i. Include any required interface cards (LON, BACnet, or other)
ii. Programming of DDC controls
11. HVAC and electrical permits
12. Start up and test operation
13. One (1) year warranty parts and labor
14. Three (3) year material-only warranty on coils
15. Five (5) year material-only warranty on compressor(s)
16. Ten (10) year material-only warranty on heat exchanger(s)
17. Any applicable taxes included in price

General Scope Clarifications:

1. Reusing existing thermostats inside of building or provide alternate price for new thermostat
2. Re-use existing electrical disconnect and GFI or provide alternate for new
3. Existing equipment is to be removed and replaced the same day and to provide heating or cooling prior to the next day

Exclusions:

1. Overtime or work performed outside of normal working hours.
2. Painting or patching any surfaces new to or on the existing building structure
3. Temporary heating or cooling

Price:

Dollars	$.00

Add for:

Optional Accessory or Feature	$.00

