ABC, Inc. 
Milwaukee, WI 
REQUEST FOR PROPOSAL
LOW VOLTAGE WIRING

1. Summary
ABC is seeking bids for indoor Low Voltage – Voice/Data cabling components to be placed
within building. In the building, the cable will integrate with existing networking
equipment.
2. General Instructions
2.1 Pre-Bid Vendor Meeting
A Pre-Bid Vendor Meeting is scheduled for XXX
This meeting will be held at:
ABC
Street Address 123
Milwaukee, WI 53051
*This meeting is not mandatory.
2.2 Due Date and Location
Proposals are due no later than 00/00/0000 Late responses will not be
considered.
Submit responses to:
ABC
Attn: Facilities Manager
Street Address 123
Milwaukee, WI 53051

2.3 Number of Copies
Three (3) copies of your completed proposal should be submitted.
2.4 Vendor Contact
The response to this RFP must name one person to be the coordinator for your RFP
response and for any clarification activities that might be necessary. Complete contact
information must be provided.
2.5 Clarification of Proposal
ABC reserves the right to obtain clarification of any point in a vendor’s proposal or to
obtain additional information necessary to properly evaluate a particular proposal.
Failure of a vendor to respond to such a request for additional information or
clarification may result in rejection of a vendor’s proposal.
Vendors may also request clarification to any part of this document by sending their
request to the aforementioned email address. Points of clarification requested by a
vendor will be sent to all vendors.
2.6 Format of Proposal
For ease of finding required information the proposal is to follow precisely the order
and section number format of this RFP. Other materials not directly related to the
stated requirements are to be included in the appendices.
The proposal should include a contract for all proposed services. 
2.7 Equipment Requirements
The vendor should propose an equipment configuration that matches the specified
requirements. The equipment must have technical support available during normal
business hours and should have extended support after business hours if ABC so
desires.
2.8 Support Requirements
Support requirements are specified in Section 6. The proposal should specifically
address each requirement listed.
2.9 Warranties
Vendor must provide warranty coverage information for all equipment. Include
applicable starting and ending periods of all warranties.
2.10 Vendor Background/Requirements
Company Information
1. List your company’s legal name, address, and telephone number. Include parent
company information if applicable.
2. How long has your company been in business?
3. How long has your company or division been providing cabling services?
2.11 References
Provide a minimum of three (3) references for customers with operations similar to
Fayette County Schools that your company has worked with in the past two years.
Include contact names, telephone numbers, and addresses. 
By submitting a proposal the vendor agrees that ABC may contact any references
enclosed in the submitted proposal.
2.12 Delivery and Implementation Schedule
Implementation and delivery of materials and work will be agreed upon by ABC and
the vendor.  All equipment and labor should be finished before this time. Any labor required after the school is open will be
at ABC’s discretion and will be discussed with the vendor.
2.13 Evaluation Criteria
The following general criteria will be used to evaluate the responses:
1. Ability of the equipment and services to meet ABC’s general and specific
integration requirements, as shown in the request, and verified by references
and/or functional demonstration.
2. Vendor’s ability to support the requested equipment determined by the
following:
a. Availability to directly communicate with technical support members.
b. The location of technical support.
c. The quality of support received in the past or the testimony from the
vendor’s supplied references.
d. Level, quality and type of client training and technical assistance provided.
e. Results of reference checks and on site/off site demonstrations.
f. Total cost, which considers both initial acquisition and ongoing operation
costs.
g. Upward compatibility for future growth.
h. Ease of use and operation of the system according to ABC’s general and
specific requirements.
3. Project Scope of Work and Pricing Options
This project shall consist of two (2) services:
1. Termination, toning and punch downs of installed cables at network drop locations
and at server rack locations.  Patch Panels shall be clearly labled. 
[bookmark: _GoBack]2. Sale and installation of network cabling.  All cables to be labeled at both points of termination.
3. Testing of all cables 
4. An as built drawing 

4. Required Equipment (See attached spec sheet)
The vendor should ensure that detailed equipment specifications are provided including the
physical dimensions of each product. See attached Spec sheet.
5. Installation
5.1 Bidder will assume installation and configuration during hours of 7:30 A.M. to 5:00
P.M. Central Time, Monday through Friday. Other arrangements may be possible, if
mutually agreeable.
5.2 Work shall be scheduled and executed in a manner to avoid as much interference as possible with normal operations of the school building. Corridors, stairs, and other exit ways shall remain in use and kept passable and free of debris and stored materials at all times.
5.3 Vendor will provide a detailed site survey for the location in coordination with
Technology Coordinator prior to purchase and implementation, at which time specific
access point locations will be agreed upon by vendor and customer.
5.4 Installation must conform to all building and electrical codes including the use of
plenum-rated cables in plenum-rated air spaces.
5.5 No alternates or substitutions of equipment, materials, or other items are allowed
without the written consent of.
5.6 Contractor assumes responsibility of assuring all installation is in working order and
approved by ABC by mutually agreeable project deadline.

6. Support Requirements
6.1 Equipment Delivery
The vendor must supply an expected delivery schedule of all equipment and accessories.
6.2 Equipment Documentation
The vendor is required to provide all documentation in either a printed or electronic
copy. The vendor should also include any performance specification and throughput
ratings, both maximum and standard, that are available for each product.
6.3 Product Support
The vendor must provide FCS with a complete list of equipment and accessories
which are covered under maintenance warranties. The vendor should also include
methods of contacting product support. The vendor should also include the various
levels of support and the processes required to escalate a case if necessary or relevant.
Documentation of renewing maintenance contracts will also be required in the
vendor’s proposal.


Parts List:
ABC
100 total Cat 6 drops between MDF and Data locations
3 Cat 6 48 port loaded patch panels
100 Cat 3 Jacks 
1 IT enclosure 19U
